
Description of the demo database 'EKS Light Application':
(EKM DB - EKS Light OS-0 OS-1 - Status 02-09/10)

This demo database serves for parameterization of the Electronic-Keys for the EKS Light application. It is possible to parameterize the Keys for the operating state 0 and operating state 1. After input of the data and activation of the 'Write' command, an EKS Light data block including check-sum (CRC) is written onto the key. After installation proceed as follows.


Logon

The istalled user is:

User                    Password

ekm                     ekm


The parameterization of the Key is to be applied in the following sequence:

1. Choose desired value of the Operating State OS.
2. Input desired Access Code AC according to DIP switch nomenclature (2.1 to 2.10) in binary mode.
3. It is absolutely necessary to set the Reserve bits R to OFF.
4. Choose desired Access Level AL.
5. Additional administrate inputs like employee names, issue date or remarks are optional and not necessary for the function of EKS Light. Those data are stored only in the database on the PC.
6. Write data on the key.